General Internet Video Card

In Setup menu, in General tab you can find general information like:

- The name and patf of log file;
- Log Level: in log file there are information about the errors apear during the soft running, warnings, etc . You can set that in log file to be raported just errors (ERROR), or just warnings (WARNING) or both type of information.(DEBUG). There are more level of errors (depands of error sternness): DEBUG, DEBUG+, DEBUG++;

- The foder where it save the recordings. You can set the minimum free space on the harddisk.The soft record images from cameras until the limit you've specified, after that it delete the oldest records;

- The folder where it save the pictures (you can set the quality of images);
- If your hard-disk space is limited you can set thet the soft delete the oldest pictures;
- Maximum numbers of inputs;
- The languageLimba in care sa ruleze programul;
- To launch ZSK on start up check Launch ZSK on startup;
- To display warnings about the soft running, select Show Warnings;
- To run ZSK in full screen mode chech Full Screen;

Back

The setings for broadcast are in Internet page.

You must fill in:

- Computer IP;
- Maximum number of clients that can view the image on internet, simultaneous;
- Portul TCP;

For Dial-up networking there are the following options:

- ISP - is dial-up connection
- User name and password to login for viewing images;
- Phone number for dial-up connection;
- If you want to dial-up on start up select Viewer mode - dial-up on start;
- For manual connect/disconnect (using dial-up) use Connect/Disconnect buttons. To view the connection information use Status button.

Back

In Video card page you can fill in the settings for video cards. It can be use maximum 4 devices simultaneous. For each video card use "Set" button, from list select an existing card.

After card selection, you can specify the parametrs (in Proprieties window): image size, video standard (NTSC, PAL N, PAL BDGHI, PAL M, SECAM), fps. You can activate watch dog option (available for HICAP cards); this option reset the computer when it crash (the watch dog wire from video card is connect to reset.

You can modify video codec (available on your computer) used for compresing the images and compression rate.

Back